/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\*@brief for TLSR chips


\* @date March 29, 2021

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/


**Patch for Flash driver and low voltage detection: used for “telink\_sig\_mesh\_sdk” SDK version V3.3.2 and prior.**

In order to update patch, you need to do the following things:


1. **Update flash driver：**
2. replace file " **\proj\drivers\flash.c** , **flash.h**"
3. add folder "**\drivers\8258\flash**" to path "\**drivers\8258**”
4. add "**\drivers\8258\flash\_mesh\_extend.c**" to path "**\drivers\8258**”
5. update file " **\proj\mcu\ compiler.h**" to add define of “\_attribute\_ram\_code\_sec\_” and “\_attribute\_ram\_code\_sec\_noinline\_”




1. **Add low voltage detection function：**
2. replace file " **\drivers\8258\ adc.c, adc.h**", " **\drivers\8278\ adc.c, adc.h**"
3. add " \vendor\common\battery\_check.c, battery\_check.h, battery\_check\_827x.c" to path "\**vendor\common\**”
4. update "proj\_lib\ble\blt\_config.h” to add "LOW\_BATT\_FLG” and “LOW\_BATT\_LOOP\_FLG”




1. update " vendor/common/light.c” to add "|BIT(LOW\_BATT\_FLG)” and “|BIT(LOW\_BATT\_LOOP\_FLG)” as shown below:





1. update " vendor/common/mesh\_common.h” to add “#include "battery\_check.h"



1. update to add define of “BATT\_CHECK\_ENABLE” and IO setting into

firmware/vendor/boot\_loader/app\_config\_8258.h

firmware/vendor/boot\_loader/app\_config\_8278.h

firmware/vendor/mesh/app\_config\_8258.h

firmware/vendor/mesh/app\_config\_8278.h

firmware/vendor/mesh\_gw\_node\_homekit/app\_config\_8258.h

firmware/vendor/mesh\_lpn/app\_config\_8258.h

firmware/vendor/mesh\_lpn/app\_config\_8278.h

firmware/vendor/mesh\_provision/app\_config\_8258.h


firmware/vendor/mesh\_provision/app\_config\_8278.h

firmware/vendor/mesh\_switch/app\_config\_8258.h

firmware/vendor/mesh\_switch/app\_config\_8278.h

firmware/vendor/spirit\_lpn/app\_config\_8258.h

firmware/vendor/spirit\_lpn/app\_config\_8278.h



1. update to add function calling of “app\_battery\_power\_check\_and\_sleep\_handle(1);” in all main\_loop(), and “app\_battery\_power\_check\_and\_sleep\_handle(0);” at the first of all user\_init(). Include:

firmware/vendor/mesh/app.c


firmware/vendor/mesh\_gw\_node\_homekit/app.c


firmware/vendor/mesh\_lpn/app.c

firmware/vendor/mesh\_provision/app.c

firmware/vendor/mesh\_switch/app.c

firmware/vendor/spirit\_lpn/app.c





1. update “\vendor\boot\_loader\main.c” to add function calling of “app\_battery\_power\_check\_and\_sleep\_handle(1);” and “app\_battery\_power\_check\_and\_sleep\_handle(0);”

